1. True / False: Samples only need to be maintained under chain-of-custody in the field.
2. True / False: Do not enter underground locations to collect samples.
3. Multiple Choice: A tailgate safety meeting should always be:   
   \_\_\_ A. held before commencing work at the site  
   \_\_\_ B. conducted daily, to discuss the activities and potential hazards/concerns  
   \_\_\_ C. held every hour  
   \_\_\_ D. Answers A&B only   
   \_\_\_ E. Answers A, B, &C

1. True / False: Visual inspection of stormwater is an inexpensive way of detecting the presence of pollutants affecting the appearance of the discharge.
2. True / False: Airport are always issued Individual permit tailored to facility and activities.
3. True / False: Runoff from construction projects at airports does not impact stormwater quality.
4. Multiple Choice: Stormwater samples are generally collected at a location \_\_\_\_\_\_ the stormwater leaving the facility and \_\_\_\_\_\_\_\_\_ all industrial materials and activities that could introduce pollutants into runoff.   
   \_\_\_ A. after, upstream  
   \_\_\_ B. prior to, the location where  
   \_\_\_ C. away from where, upstream to  
   \_\_\_ D. prior to, downstream from
5. Multiple Choice: Common objectives for airport stormwater monitoring include:  
   \_\_\_ A. Industrial Stormwater Permit Compliance   
   \_\_\_ B. Deicer Runoff Management  
   \_\_\_ C. Construction Permit Compliance  
   \_\_\_ D. All of the above
6. Multiple Choice: Planning documentation for field sampling programs include:  
   \_\_\_ A. Work Plan and Sampling and Analysis Plan  
   \_\_\_ B. Quality Assurance Project Plan   
   \_\_\_ C. Health and Safety Plan  
   \_\_\_ D. All of the above
7. True / False: Composite sampling consists of a collection of numerous individual discrete samples taken at regular intervals over a period of time.